
  STE background audio player
  Spar (Spare, Spartanic) version.

  WAV format supported:
  8-bit PCM, stereo, 50066 Hz

  First time by clicking on Play/Stop open
  WAV file made with parameters above
  ( on PC  with some SW ) - program will
  convert it to WAE file, what will than
  play with minimal system load on STE.
  Conversion self may take couple minutes,
  what depends on WAV duration and hard
  disk speed.
  Of course,  may immed. delete  src.
  WAV file. when conversion is done.

  Klick again on Play/Stop and select WAE
  file - playback will start immed.

  May set volume with arrows lower - 
 - on STE and TT, works not on Falcon.

  There are limitations what is possible to
  do without crash and other troubles:

  Possible is:  running regular GEM SW
 as diverse editors, database handlers etc.  
 Graphic programs what use not special tricks
  - Degas will work. Spectrum 512 and
  other like ones not.

  Do not run:  games, debuggers, system
   affecting SW and similar. It is not
   enough to just stop playback 
  - you need to restart with deactivated ACC .

  Do not try to change Desktop resolution
  - it will crash. If need different res, must
   deactivate ACC and reset Atari.
   Then Save Desktop in wanted res.
   and activate back ACC, and reset again.
 
  This is alpha 0.45 version.  
  Works on STE, TT & Falcon. Hard disk
  is mandatory.  Transfer rate during playback
  is about 100 KB/sec.


  Peter Putnik , March  14   2011.



  