
     Hi-Color  Video player for Atari STE 
     Res:  320x78px  25  fps


  Preliminary versions of this player. First release.
Made for real Atari STE HW, equipped with popular UltraSatan
mass storage adapter.

  Requirements:
RAM - 512KB. Free RAM - 200KB.
Atari STE. It will work on some ST too, but without sound
and less colors - some parts may look ugly.
Fast mass storage -  min transfer rate is 1100KB/sec.
Additionally, access time must be fast too. My 4GB
Quantum SCSI drive has over 1200KB/sec, but is not
good - because slower access times. So, the best choice
is UltraSatan. But not all SD cards can achieve that speed.
So, please do some speed tests if playback is not OK.
Defragmented partition on which will copy long AV file.
It is a must, because speed is essence here, and we know
that fragmented files load slower.

Limitations:
P158SI works with any ACSI target # 0-7. From any location
on disk, so may copy to any partition. Works with DOS partitioned
disks too, where BigDOS SW is used. Of course, still need to
defragment.
Because using ICD command set, this works not with emulators.

P158SR works with ACSI target 0, HAV file must be in first GB of disk.
Works with emulators too, but only real hard disk emulation with
image file.

You must not type extension (HAV). Filename self is enough.
Like SNO or EN1 here.


P158SE - for emulators and GEMDOS type hard disk emul. -
- so from PC DIR as Atari logical drive.

Tested with PP, AHDI, ICD and Hddriver. Driver speed self
is not relevant, because this uses own, fast direct ACSI
port disk reading code (only way to get enough reading speed).



Future plans:
Support of IDE hard disks - actually, Compact Flash cards
via IDE IF - then can have even better quality. Write me
mail, or post in forum if interested about it. Please describe
your HW - what IDE IF, CF card have.

P. Putnik,  27 Dec 2012.
