¡l
        Test V909  Please wait for sanity checks to complete.
        Press any key to abort automated Functional Test.
 
        CD Module ROM checksum is $366c 
 
        Test Suites completed = 003e 
 
        Last test started = 007a 
 
        Quick-check completed with no problems.
 
        Test 6.3.7 EEPROM write / read-back                     passed!
        Test 6.3.7 EEPROM write / read-back                     passed!
        Test 6.3.2A FFFF/0000 words serial data test            passed!
        Test 6.3.2B Dual-counter serial data test               passed!
        Test 6.3.2C Butch FIFO to Tom 32-bit data test          passed!
        Test 6.3.4 Decreasing span seeks speed test             passed!
        Test 7A. Hole-in-CD playability test
                Try playing the drop-out.
                Information layer drop-out tolerance OK.
                Try playing the 600 uM dot.
                Played the 600 uM black dot OK.
                CIRC failure-detection works OK.

                Self-tests PASSED.  Congratulations!
                External evaluation required for the following tests:

 
        Test 4.4.9 BLER.  Requires connection to Jag Tester!
        No BLEREVAL UNIT detected.
        Press any key to continue.
 
        UUT now playing track 50.
 
        UUT played track OK.
 
        Test 9  Film clip playback.
0001    = Number, in hex, of film loops started
                Cinepak program ended normally
 
 
  Film playback terminated. Open the lid to verify that reset works.
 
        Lid test detected.

                DSA error #042c 
 
        Unit PASSED!

