        Jaguar CDROM Test V915

        >>>PLEASE WAIT FOR SANITY CHECKS TO COMPLETE<<<

        Test 01  CD Module ROM checksum is $2d21

        Test Suites completed = 0000
        Last test started = 0000
 
        Test 02  Initial sanity check                 PASSED!
        Test 03  EEPROM write/read-back               PASSED!
        Test 04  Subcode channel                      PASSED!
        Test 05  FFFF/0000 words serial data          PASSED!
        Test 06  Dual-counter serial data             PASSED!
        Test 07  Butch FIFO 32-bit data               PASSED!
        Test 08  Decreasing span seeks                PASSED!
        Test 09  Playing the drop-out                 PASSED!
        Test 10  Try playing the 600 uM dot           PASSED!
        Test 11  CIRC failure-detection               PASSED!

        >>> EXTERNAL EVALUATION REQUIRED FOR THE FOLLOWING TESTS<<<

        Test 12  BLER. track 50                       PASSED!
        Test 13  Film clip playback.                  PASSED!

        >>> OPEN THE LID TO VERIFY THAT RESET WORKS <<<

       Test 14        Lid test detected              
        DSA error #042c

       !! UNIT PASSED !!






























        Jaguar CDROM Test V915

        >>>PLEASE WAIT FOR SANITY CHECKS TO COMPLETE<<<

        Test 01  CD Module ROM checksum is $2d21

        Test Suites completed = 0000
        Last test started = 0013
 
        Test 02  Initial sanity check                 PASSED!

        Jaguar CD Module Functional Test V915   20 October 1995

                                MAIN MENU

        Please select an item by letter.
        (B) BLER test
        (C) Current and voltage tests on PCBA
        (D) Data integrity tests using Jerry then Tom
        (E) EEPROM write and read-back test
        (F) Film clip playback
        (H) Hole-in-CD tolerance test.
        (J) Jitter tests
        (L) Loop control of tests
        (R) Read and evaluate serial data quality
        (S) Seeks of decreasing spans tests
        (V) V4 Subcode test


        Waiting ....
        Number of data test loops completed = $00000002
        DSA error #042c

        DSA error #042c

        DSA error #042c
 
        DSA error count  = $00000001 
        DSP buff timeout = $00000000 
        CIRC error count = $00000000 
        Data error count = $00000000 
        UFOs error count = $00000000 
        Number of data test loops completed = $00000003
        DSA error #042c

        DSA error #042c

        DSA error #042c

        DSA error #042c
 
        DSA error count  = $00000002 
        DSP buff timeout = $00000000 
        CIRC error count = $00000000 
        Data error count = $00000000 
        UFOs error count = $00000000 
        Number of data test loops completed = $00000004
