HPI_DMACtl_ADR at C0C0 -- is this the HPI DMA address?
	Probably not -- it says something about DREQ, D0, D1...hmm.
EZ-OTG can run the 'Flash' bus on GPIO
There are also modes for boundary scan and EPP and so on
