
bjbugs/jserve	Windows application to connect GDB to the Jaguar
bjbugs/jdb	Jaguar debugging stub, auto-loaded by jserve
boot/		JagUSB boot block, plus COF file to unlock/re-flash the boot block
		If you screw up, you can always use BJL to re-run the original COF
butcher/	VHDL source code for 'Butcher', my nickname for the CPLD
flash/		Jaguar COF file to Flash an Alpine ROM image
jcp2/		Windows application that talks to boot/ or flash/ via USB
pcb/		FreePCB source files for the Jag USB PCB
		manufacture.zip is the exact file that I sent to manufacture your board
turbow/		EZ-HOST code that allows jcp2/ to write into Jag memory via USB
		This is used by jcp2/ and bjbugs/jserve
