### Summary

Design Name | main
Fitting Status | Successful
Software Version | J.37
Device Used | XC9572XL-10-VQ64
Date | 8- 8-2007, 4:36PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
44/72 (62%) | 88/360 (25%) | 4/72 (6%) | 42/52 (81%) | 64/216 (30%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 3 | 3
Output | 7 | 7
Bidirectional | 32 | 32
GCK | 0 | 0
GTS | 0 | 0
GSR | 0 | 0
Pin Type | Used | Total
--- | --- | ---
I/O | 39 | 46
GCK/IO | 1 | 3
GTS/IO | 1 | 2
GSR/IO | 1 | 1

##### GLOBAL RESOURCES

Global clock net(s) used | 0
Global output enable net(s) used | 0
Global set/rest net(s) used | 0

##### POWER DATA

Macrocells in high performance mode (MCHP) | 0
Macrocells in low power mode (MCLP) | 44
Total macrocells used (MC) | 44